Final Fit-Out Verification Checklist
Use this checklist to systematically verify every finish item in your home room by room. This walkthrough happens after trim, doors, paint, lighting, plumbing fixtures, and hardware are installed. Think of it as your pre-punch-list review — catching issues now keeps the formal punch list focused and efficient.

	Project Title: _____________________________
	Date: _____________________________



	Inspector/Observer: _________________________
	Date: _________________________


Section 1: Whole-House Trim & Paint
	Item
	Acceptable (Y/N)
	Notes

	Base trim profiles match specification throughout
	
	

	Casing/architrave profiles consistent at all doors and windows
	
	

	Crown molding (if specified) tight to ceiling and wall with smooth miters
	
	

	All trim joints tight (no visible gaps at miters or butt joints)
	
	

	Caulk applied at trim-to-wall and trim-to-ceiling joints
	
	

	Paint color correct per approved color schedule
	
	

	Paint finish even with no drips, runs, sags, or holidays (missed spots)
	
	

	Sheen level consistent by room (e.g., satin trim, matte walls, semi-gloss wet areas)
	
	

	Touch-up paint applied after cabinet, fixture, and hardware installation
	
	


Section 2: Interior Doors
	Item
	Acceptable (Y/N)
	Notes

	Door style and material match specification
	
	

	Doors swing in correct direction per plan
	
	

	Doors open and close smoothly without dragging on floor or frame
	
	

	Latch engages cleanly with striker plate (no force required)
	
	

	Hinges tight with no sagging
	
	

	Consistent reveal (gap) around door to frame (even top, sides, and bottom)
	
	

	Doorstops installed (wall or floor mount per spec)
	
	

	Privacy locks on bathrooms and bedrooms function correctly
	
	

	Glass panels (if any) match spec and are free of defects
	
	


Section 3: Room-by-Room Fixture Verification
Walk each room and check every installed item. Use one row per room.
	Room
	Lights Work
	Outlets Work
	Switches Work
	Plumbing Fixtures Installed & Tested
	Hardware Installed
	HVAC Registers in Place

	Entry/Foyer
	
	
	
	
	
	

	Living/Great Room
	
	
	
	
	
	

	Kitchen
	
	
	
	
	
	

	Dining Room
	
	
	
	
	
	

	Primary Bedroom
	
	
	
	
	
	

	Primary Bathroom
	
	
	
	
	
	

	Bedroom 2
	
	
	
	
	
	

	Bedroom 3
	
	
	
	
	
	

	Bedroom 4
	
	
	
	
	
	

	Bathroom 2
	
	
	
	
	
	

	Bathroom 3
	
	
	
	
	
	

	Powder Room
	
	
	
	
	
	

	Home Office
	
	
	
	
	
	

	Laundry
	
	
	
	
	
	

	Mudroom
	
	
	
	
	
	

	Garage
	
	
	
	
	
	

	Hallways
	
	
	
	
	
	

	Closets
	
	
	
	
	
	

	Exterior — Front
	
	
	
	
	
	

	Exterior — Back
	
	
	
	
	
	

	Exterior — Side
	
	
	
	
	
	


Section 4: Hardware Schedule Verification
	Hardware Item
	Finish per Schedule
	Installed Finish
	Match? (Y/N)
	Notes

	Interior door levers/knobs
	
	
	
	

	Exterior door hardware (entry set, deadbolt)
	
	
	
	

	Cabinet pulls — kitchen
	
	
	
	

	Cabinet knobs — kitchen
	
	
	
	

	Cabinet hardware — bathrooms
	
	
	
	

	Towel bars/rings
	
	
	
	

	Toilet paper holders
	
	
	
	

	Robe hooks
	
	
	
	

	Shower door handles
	
	
	
	

	Window locks and operators
	
	
	
	


Hardware finish inconsistency is one of the most common (and most visible) oversights at this stage. Verify every piece against the approved schedule.
Section 5: Plumbing Fixture Testing
	Fixture
	Location
	Installed
	Hot/Cold Correct
	No Leaks
	Drain Working
	Notes

	Kitchen sink
	
	
	
	
	
	

	Kitchen faucet (spray, hot water, disposal switch)
	
	
	
	
	
	

	Dishwasher (run cycle)
	
	
	
	
	
	

	Primary bath sink(s)
	
	
	
	
	
	

	Primary bath tub/shower
	
	
	
	
	
	

	Primary toilet
	
	
	
	
	
	

	Bath 2 sink
	
	
	
	
	
	

	Bath 2 shower/tub
	
	
	
	
	
	

	Bath 2 toilet
	
	
	
	
	
	

	Bath 3 sink
	
	
	
	
	
	

	Bath 3 shower/tub
	
	
	
	
	
	

	Powder room sink and toilet
	
	
	
	
	
	

	Laundry sink (if applicable)
	
	
	
	
	
	

	Exterior hose bibbs
	
	
	
	
	
	


Section 6: Issues Found
	Item #
	Room
	Issue
	Category
	Resolution
	Fixed
	Verified

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	


Next Steps
Document all deficiencies and assign responsible parties for correction. Schedule a follow-up inspection to verify all items have been completed before final walkthrough and closing.
