Pre-Drywall Checkpoint Checklist
This is the single most important inspection of your entire project. Once drywall goes up, everything behind it becomes invisible and extraordinarily expensive to access. Take your time with this walkthrough. Bring your architect or an independent inspector. Check every item. This is your last chance to catch problems before they're buried in walls and ceilings.
	Project Title: _____________________________
	Date: _____________________________



	Inspection Date: _______
	Inspector(s): _______
	Builder Representative: _______



Section 1: Insulation Verification
	Item
	Verified (Y/N)
	Location/Notes
	Photo Ref

	Insulation type matches specifications for each assembly (walls, ceiling, floor)
	
	
	

	R-values match specifications (check label on installed product)
	
	
	

	Full cavity fill — no gaps, voids, compressions, or missing sections
	
	
	

	Insulation properly fitted around electrical boxes and wiring
	
	
	

	Insulation properly fitted around plumbing pipes
	
	
	

	No insulation stuffed behind pipes (should wrap around, not compress)
	
	
	

	Baffles installed at eave vents to maintain airflow
	
	
	

	Band/rim joist insulation installed
	
	
	

	Vapor barrier orientation correct for climate zone (warm side)
	
	
	



Section 2: Air Sealing Verification
	Item
	Verified (Y/N)
	Location/Notes
	Photo Ref

	Top plates sealed (caulk, foam, or gasket at wall-to-ceiling connection)
	
	
	

	Bottom plates sealed at wall-to-floor connection
	
	
	

	Electrical box penetrations sealed (foam, putty pads, or gaskets)
	
	
	

	Plumbing penetrations sealed
	
	
	

	HVAC penetrations sealed
	
	
	

	Recessed light fixtures air-tight rated (IC-AT) or sealed
	
	
	

	Duct penetrations through conditioned envelope sealed
	
	
	

	Band/rim joist air sealed
	
	
	

	Fireplace chase sealed at top and bottom
	
	
	

	Bath fan and kitchen exhaust duct boots sealed
	
	
	



Section 3: Rough-In Systems Verification
	Item
	Verified (Y/N)
	Location/Notes
	Photo Ref

	Electrical rough-in inspection passed
	
	
	

	Plumbing rough-in inspection passed
	
	
	

	Mechanical (HVAC) rough-in inspection passed
	
	
	

	Low-voltage wiring pulled (network, speaker, security, smart home)
	
	
	

	HVAC ductwork installed and connected
	
	
	

	Duct joints sealed with mastic (not just tape)
	
	
	

	Supply and return register locations match HVAC plan
	
	
	

	Thermostat wiring at designated locations
	
	
	

	Bathroom exhaust fans ducted to exterior (not into attic)
	
	
	

	Dryer vent ducted to exterior with proper termination
	
	
	



Section 4: Framing Corrections & Blocking
	Item
	Verified (Y/N)
	Location/Notes
	Photo Ref

	All framing inspection corrections completed and re-inspected
	
	
	

	Blocking installed for wall-mounted TV locations
	
	
	

	Blocking for bathroom grab bars (current or future)
	
	
	

	Blocking for heavy mirrors and shelving
	
	
	

	Blocking for cabinet mounting
	
	
	

	Blocking for stair railing connections
	
	
	

	Blocking for shower glass and doors
	
	
	

	Fire blocking installed at all required locations
	
	
	



Section 5: Third-Party Testing
	Test
	Scheduled?
	Date
	Result
	Pass/Fail

	Blower door test (air tightness)
	
	
	
	

	Thermal imaging scan (insulation continuity)
	
	
	
	

	Duct leakage test (if required)
	
	
	
	

	Any other required energy code testing
	
	
	
	



Blower door result: _______ ACH50 (Target: _______ ACH50)

Thermal imaging — areas of concern identified:



Section 6: Final Walkthrough — Room by Room
	Room/Area
	Insulation Complete
	Air Sealed
	Blocking Installed
	Rough-Ins Verified
	Issues

	Primary Bedroom
	
	
	
	
	

	Primary Bathroom
	
	
	
	
	

	Bedroom 2
	
	
	
	
	

	Bedroom 3
	
	
	
	
	

	Bedroom 4
	
	
	
	
	

	Bathroom 2
	
	
	
	
	

	Bathroom 3
	
	
	
	
	

	Kitchen
	
	
	
	
	

	Living/Great Room
	
	
	
	
	

	Dining Room
	
	
	
	
	

	Home Office
	
	
	
	
	

	Laundry
	
	
	
	
	

	Mudroom
	
	
	
	
	

	Garage (conditioned boundary)
	
	
	
	
	

	Attic (at ceiling line)
	
	
	
	
	

	Basement/Crawlspace
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	



Section 7: Issues & Resolution
	Item #
	Location
	Issue
	Priority (Must Fix / Should Fix)
	Responsible
	Resolved
	Verified

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	

	
	
	
	
	
	
	



Red Flag: Do NOT approve drywall installation until every 'Must Fix' item is resolved and verified. There are no second chances with this inspection.

Sign-Off
All items verified and approved for drywall?
☐ Yes   ☐ No — see open items above
Owner/Inspector signature: _________________________   Date: _____________

Builder acknowledgment: _________________________   Date: _____________

Next Steps
After completing this inspection and resolving all issues, the next critical phase is proceeding with drywall installation and interior finishing.
