Module 3 Lesson 8
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Infrastructure Coordination Checklist
Use this checklist to ensure that lighting, audio-visual, and landscape elements are planned as infrastructure — not treated as last-minute finish selections. These systems require wires, pipes, conduit, and concrete footings that must be coordinated during design and roughed in during framing, not after drywall.
Project Title: _________________________________________________________________
Date: _________________________________________________________________
Part 1: Lighting Infrastructure
	Item
	Design Phase Required
	Responsible Party
	Specified
	Coordinated with Structure/MEP
	Notes

	Lighting concept/zones defined (ambient, task, accent)
	
	
	
	
	

	Fixture locations marked on reflected ceiling plan
	
	
	
	
	

	Switch and dimmer locations mapped
	
	
	
	
	

	Circuit requirements and panel capacity confirmed
	
	
	
	
	

	Recessed fixture clearances verified (insulation contact rating)
	
	
	
	
	

	Under-cabinet and toe-kick lighting conduit
	
	
	
	
	

	Exterior fixture locations and conduit runs
	
	
	
	
	

	Landscape lighting transformer location and low-voltage runs
	
	
	
	
	

	Dimming system / smart lighting protocol selected
	
	
	
	
	

	Emergency/egress lighting (if required by code)
	
	
	
	
	



Part 2: Audio-Visual & Technology Infrastructure
	Item
	Design Phase Required
	Responsible Party
	Specified
	Coordinated with Structure/MEP
	Notes

	Structured wiring plan (Cat6/fiber runs to each room)
	
	
	
	
	

	WiFi access point locations and power/data drops
	
	
	
	
	

	In-wall/ceiling speaker locations and wiring
	
	
	
	
	

	Equipment closet/rack location with power, ventilation, and access
	
	
	
	
	

	TV locations with power, data, and conduit behind wall
	
	
	
	
	

	Outdoor speaker and camera locations with conduit
	
	
	
	
	

	Intercom/video doorbell pre-wire
	
	
	
	
	

	Motorized shade pockets and power (if applicable)
	
	
	
	
	

	Security system pre-wire (sensors, keypads, panel)
	
	
	
	
	

	Conduit for future technology runs (spare conduit paths)
	
	
	
	
	



Part 3: Landscape Infrastructure
	Item
	Design Phase Required
	Responsible Party
	Specified
	Coordinated with Structure/MEP
	Notes

	Hardscape areas requiring footings or structural support (pergola, outdoor kitchen, fire pit)
	
	
	
	
	

	Irrigation main line routing and zone design
	
	
	
	
	

	Exterior drainage integration (French drains, dry wells, swales)
	
	
	
	
	

	Pool/spa equipment pad location with utilities (electrical, gas, water)
	
	
	
	
	

	Outdoor kitchen utilities (gas, water, electrical, drain)
	
	
	
	
	

	Exterior lighting conduit and transformer pad
	
	
	
	
	

	Gate/fence automation power and controls
	
	
	
	
	

	Retaining wall engineering (if height requires)
	
	
	
	
	

	Site grading coordination with building pad
	
	
	
	
	

	Root barrier and tree protection during construction
	
	
	
	
	



Conflict Check Summary
	System
	Potential Conflict With
	Resolution / Coordination Required
	Resolved?

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	



Red Flag:
Any item marked "Not Specified" after Design Development is at risk of being missed during construction or requiring expensive change orders. Escalate unresolved items to your architect immediately.
Next Steps
1. Review each infrastructure system during the Design Development phase.
2. Assign responsibility for each item to your design team (architect, engineer, or specialist).
3. Identify and resolve all conflicts before moving to Construction Documents.
4. Use this checklist during Constructability Review to confirm all systems are ready for rough-in.
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